Vision Rack
VSR 800
INPUT		
Rated power	800 VA	
Voltage	220 / 230 / 240 V 	
Frequency	50 / 60 Hz with automatic selection 	
Frequency tolerance	±5% Hz (3% to 10% conﬁgurable)	
OUTPUT and INVERTER OUTPUT		
Rated power	800 VA	
Active power	640 W	
Waveform	Sinusoidal 	
Frequency	50 or 60 Hz with automatic selection 	
BATTERIES		
Type	VRLA AGM maintenance-free lead based 	
Typical recharge time	4-6 h 	
ENVIRONMENTAL		
Color	Black 	
Protections	Overload - short circuit - overvoltage - undervoltage - temperature - excessive low battery	
Noise (at 1 m)	<50 [dBA] 	
Operating temperature	0 °C - +40 °C	
Relative humidity	5-95% non-condensing	
Output sockets	4 IEC 10A 	
Standards	European directives: L V 2014/35/EU low voltage; EMC 2014/30/EU electromagnetic compatibility -- Directive and Standards: Safety IEC EN 62040-1; EMC IEC EN 62040-2; RoHS compliant 	
DATA		
Weight	12 kg	
Dimensions (h w d)	1Ux19"x420 mm